| TUCSON(LM) >2012 > G 2.4 DOHC > Heating,Ventilation, Air Conditioning > Blower > Blower Unit>Repair procedures |

Replacement
1. | Disconnect the negative (-) battery terminal.
2. | Remove the crash pad. (Refer to BD group-crash pad)
3. | Remove the cowl cross bar assembly. (Refer to BD group-crash pad)
4. | Remove the heater and blower unit. (Refer to HA group-crash pad)
5. | Remove the blower unit (A) from the heater unit after loosening a mounting bolt and 3 screws.
Make sure that there is no air leaking out of the blower and duct joints.
6. | Installation is the reverse order of removal.