| TUCSON(LM) >2012 > G 2.4 DOHC > Engine Mechanical System > Intake And Exhaust System > Intake Manifold>Repair procedures |

Removal and Installation
1. | Disconnect the battery negative terminal (A).
Tightening torque: (-) terminal : 4.0 ~ 6.0N.m (0.4 ~ 0.6kgf.m, 3.0 ~ 4.4lb-ft)
2. | Remove the engine cover (B).
3. | Remove the air duct (C).
4. | Disconnect the breather hose (A), air intake hose (B) and then remove the air cleaner assembly (C).
Tightening torque Hose clamp bolt: 2.9 ~ 4.9N.m (0.3 ~ 0.5kgf.m, 2.2 ~ 3.6lb-ft) Air cleaner assembly bolts: 7.8 ~ 11.8N.m (0.8 ~ 1.2kgf.m, 5.8 ~ 8.7lb-ft)
5. | Loosen the drain plug (A), and drain the coolant. Remove the radiator cap to speed draining.
6. | Remove the radiator upper hose (A).
7. | Disconnect the OCV connector (A).
8. | Disconnect the VIS connector (A), the oil pressure switch (B), the knock sensor connector (C), the A/C compressor switch connector (D) and the alternator connector (E).
9. | Disconnect the Injector connectors (A).
10. | Disconnect the VCM connector (A).
11. | Disconnect the ETC connector (A) and the MAP & IATS connector (B).
12. | Disconnect the PCV hose (A).
13. | Disconnect the fuel hose (A).
14. | Disconnect the brake booster vacuum hose (A), PCSV hose (B) and the throttle body coolant hoses (C).
15. | Remove the intake manifold stay (A) and then disconnect the sensor connectors from the mounting bracket.
Tightening torque : 18.6 ~ 23.5N.m (1.9 ~ 2.4kgf.m, 13.7 ~ 17.4lb-ft)
16. | Remove the intake manifold (A).
Tightening torque : Bolts & Nuts :18.6 ~ 23.5N.m (1.9 ~ 2.4kgf.m, 13.7 ~ 17.4lb-ft)
17. | Installation is reverse order of removal.