| TUCSON(LM) >2012 > G 2.4 DOHC > Suspension System > Rear Suspension System > Rear Shock Absorber>Repair procedures |

Replacement
1. | Remove the rear wheel & tire.the rear wheel & tire.
Tightening torque : 88.3 ~ 107.9N.m(9.0 ~ 11.0Kgf.m, 65.1 ~ 79.6lb-ft)
Be careful not to damage to the hub bolts when removing the front wheel & tire.
2. | Loosen the bolt & nut and then disconnect the shock absorber(A) with the rear axle.
Tightening torque : 137.3 ~ 156.9N.m(14.0 ~ 16.0Kgf.m, 101.3 ~ 115.7lb-ft)
3. | Loosen the shock absorber mounting bolts(A).
Tightening torque : 49.0 ~ 63.7N.m(5.0 ~ 6.5Kgf.m, 36.2 ~ 47.0lb-ft)
4. | Installation is the reverse of removal.
Inspection
1. | Check the rubber parts for damage or deterioration.
2. | Check the shock absorber for abnormal resistance or unusual sounds.
Disposal
1. | Fully extend the shock absorber rod.
2. | Drill a hole to remove gas from the cylinder.
The gas coming out is harmless, but be careful of chips that may fly up when drilling. Be sure to use face shield and safety goggles.