| TUCSON(LM) >2012 > G 2.4 DOHC > Body Electrical System > Button Engine Start System > Fob Holder>Repair procedures |

Removal
1. | Disconnect the negative(-) battery terminal.
2. | Remove the floor console. (Refer to the BD group - "Console")
3. | Disconnect the connector (B), then remove the fob holder assembly (A) after releasing the hook (C).
Installation
1. | Install the fob holder assembly.
2. | Install the floor console.
3. | Install the negative(-) battery terminal.