| TUCSON(LM) >2012 > G 2.4 DOHC > Engine Mechanical System > Lubrication System > Oil Cooler>Repair procedures |

Removal [2.4L Engine only]
1. | Loosen the drain plug, and drain the coolant. Remove the radiator cap to speed draining.
2. | Disconnect the oil cooler coolant hoses (A).
3. | Remove the oil filter (A).
4. | Loosen the mounting bolt (A) and remove the oil cooler assembly (B).
Installation [2.4L Engine only]
1. | Apply a light coat of engine oil to the oil cooler packing surface (A), and then Install the oil cooler with fix bolt (B).
Tightening torque: 44.1 ~ 53.9 N.m (4.5 ~ 5.5 kgf.m, 32.5 ~ 39.8 lb-ft)
Fix position of oil cooler stopper(A) where oil cooler resists on ladder frame stopper (B).
2. | Apply a light coat of engine oil to the oil filter packing surface (A), and then install the oil filter.
Tightening torque: 11.8 ~ 15.7 N.m (1.2 ~ 1.6 kgf.m, 8.7 ~ 11.6 lb-ft)
3. | Connect the oil cooler coolant hoses (B).
4. | Fill the radiator with coolant and check for leaks.