| TUCSON(LM) >2012 > G 2.4 DOHC > Body Electrical System > AVN System>Repair procedures |

Removal
1. | Disconnect the negative (-) battery terminal.
2. | Remove the hazard lamp switch assembly (A).
Take care not to damage and scratch the hazard lamp switch assembly and its related parts. Apply the protective tapes to the hazard lamp switch assembly and its related parts.
3. | Disconnect the connectors (A).
4. | Remove the center fascia panel (A).
5. | Remove the AVN assembly (A) after loosening the mounting screws.
6. | Disconnect the AVN connectors and cable (A), then remove the AVN unit completely.
When the compact disc is not ejected, do not remove it forcibly.
Installation
1. | Connect the AVN head unit connectors and cable.
2. | Install the AVN head unit.
3. | Install the center facia panel.
4. | Install the hazard switch module.
5. | Connect the negative (-) battery terminal.
Make sure the connector are connected in properly. Check the AVN system.