| TUCSON(LM) >2012 > G 2.4 DOHC > Heating,Ventilation, Air Conditioning > Air Conditioning System > Evaporator Temperature Sensor>Repair procedures |

Inspection
1. | Ignition "OFF".
2. | Disconnect evaporator temperature sensor.
3. | Using the multi-tester, Measure resistance between terminal "1" and "2" of evaporator temperature sensor. Specification
Evaporator core temperature [°C (°F)] | Resistance[KΩ]
-10 (14) | 18.01
0 (32) | 11.38
10 (50) | 7.38
20 (68) | 4.89
30 (86) | 3.33
40 (104) | 2.31
50 (122) | 1.64
Replacement
1. | Remove the console extension cover (A).
2. | Remove the left side cover (A).
3. | Remove the crash pad lower cover (A).
4. | Disconnect the diagnosis connector (A).
5. | Remove the reinforcing panel (A).
6. | Remove the shower duct (A).
7. | Remove the evaporator temperature sensor (A), by pulling it after rotating 90° in a counterclockwise direction.
8. | Installation is the reverse order of removal.