| TUCSON(LM) >2013 > G 2.0 DOHC > Body Electrical System > Immobilizer System > Antenna Coil>Repair procedures |

Removal
1. | Disconnect the negative (-) battery terminal.
2. | Remove the steering column upper and lower shrouds (A).
Take care not to damage and scratch the shrouds and its related parts. Take care not to damage the hook when removing the upper and lower shrouds.
3. | Disconnect the 6P connector (B) of the coil antenna and then remove the coil antenna (A) after loosening the screw.
Installation
1. | Install the coil antenna and connect the 6P connector.
2. | Install the steering column upper and lower shrouds.