| TUCSON(LM) >2013 > G 2.0 DOHC > Automatic Transaxle System > Valve Body System > Solenoid valve>Specifications |

Specification
Item | Function | Piece | Specification
VFS | 26/B T/Con | 2 | Control pressure: 9.81~500.14kpa (0.1~5.1kgf/cm², 1.42~72.54 psi) Current value: 50~850mA Low Type, 5.1Ω
Line pressure control | 1 | Control pressure: 500.14~9.81kpa (5.1~0.1kgf/cm², 72.54~1.42psi) Current value: 50~850mA High Type, 5.1Ω
35R UD OD | 3 | Control pressure: 500.14~9.81kpa (5.1~0.1kgf/cm², 72.54~1.42psi) Current value: 50~850mA High Type, 5.1Ω
On/Off | SS-A SS-B | 2 | Control pressure: 490.33kpa (5.0kgf/cm², 71.12psi) 10~11Ω Low Type
Solenoid Valve Operation Table
| SS-A | SS-B | UD-VFS | OD-VFS | 35R-VFS | 26-VFS
N/H | N/H | N/H | N/L
N, P | ● |  | ● |  | ● |
1 | Δ |  |  | Δ | ● |
2 |  |  |  | ● | ● | ●
3 |  | ● |  | ● |  |
4 |  |  |  |  | ● |
5 |  | ● | ● |  |  |
6 |  |  | ● |  | ● | ●
L | ● |  |  |  | ● |
R | ● | ● | ● |  |  |