| TUCSON(LM) >2013 > G 2.0 DOHC > Fuel System > Engine Control System > Crankshaft Position Sensor (CKPS)>Repair procedures |

Inspection
1. | Check the signal waveform of the CMPS and CKPS using the GDS.
Specification: Refer to “Wave Form”
Removal
1. | Turn the ignition switch OFF and disconnect the battery negative (-) cable.
2. | Disconnect the crankshaft position sensor connector (A).
3. | Remove the protector (A).
4. | Remove the installation bolt (A), and then remove the crankshaft position sensor.
Installation
• | Install the component with the specified torques.
• | Note that internal damage may occur when the component is dropped. In this case, use it after inspecting.
• | Apply the engine oil to the O-ring.
• | Insert the sensor in the installation hole and be careful not to damage when installation.
1. | Installation is reverse of removal.
Crankshaft position sensor installation bolt: 9.8 ~ 11.8 N.m (1.0 ~ 1.2 kgf.m, 7.2 ~ 8.7 lb-ft) Crankshaft position sensor protector installation bolt (M8): 18.6 ~ 23.5 N.m (1.9 ~ 2.4 kgf.m, 13.7 ~ 17.4 lb-ft) Crankshaft position sensor protector installation bolt (M6): 9.8 ~ 11.8 N.m (1.0 ~ 1.2 kgf.m, 7.2 ~ 8.7 lb-ft)