| TUCSON(LM) >2013 > G 2.0 DOHC > Automatic Transaxle System > Automatic Transaxle Control System > Inhibiter Switch>Repair procedures |

Removal
1. | Set room side lever and T/M side lever to "N" position.
2. | Remove the battery and the battery tray. (Refer to "Charging system" in EE group.)
3. | Remove the air cleaner assembly. (Refer to "Intake manifold" in EM group.)
4. | Remove the shift cable mounting nut (B).
5. | Disconnect the inhibitor switch connector (A).
6. | Remove the manual control lever (A) and the washer (B) after removing a nut (C).
When installing, fix the manual control lever and the inhibitor switch with Ø5mm (0.1969in.) fixing jig. And then tighten the inhibitor assembly mounting bolts.
7. | Remove the inhibitor assembly (A) after removing the bolts (2ea).
Tightening torque: 9.8 ~ 11.8 N.m (1.0 ~ 1.2 kgf.m, 7.2 ~ 8.7 lb-ft)
When installing, tighten the inhibitor assembly mounting bolt lightly.
Installation
1. | Installation is the reverse of removal.