| TUCSON(LM) >2013 > G 2.0 DOHC > Emission Control System > Evaporative Emission Control System > Canister>Repair procedures |

Removal
1. | Remove the fuel tank. (Refer to "Fuel tank" in FL group.)
2. | Disconnect the vapor tube quick-connector (A,B) and the ventilation hose (C).
3. | Remove the canister in the direction of an arrow after removing the installation screws (D).
Inspection
1. | Check for the following items visually. - Cracks or leakage of the canister - Loose connection, distortion, or damage of the vapor hose/tube A: Canister ↔ Atmosphere B: Canister ↔ Intake Manifold C: Canister ↔ Fuel Tank
Installation
Installation is the reverse of removal.
Canister installation bolt/nut: 3.9 ~ 5.9 N.m (0.4 ~ 0.6 kgf.m, 2.9 ~ 4.3 lb-ft)