| TUCSON(LM) >2013 > G 2.0 DOHC > Body Electrical System > Windshield Wiper/Washer > Front Wiper Motor>Repair procedures |

Removal
1. | Remove the windshield wiper arm and blade after removing a nut (B) and wiper cap (A).
2. | Remove the windshield wiper arm and blade (A) after removing a nut.
3. | If necessary, release the wiper blade fixing clip by pulling up and remove the wiper blade from the inside radius of wiper arm.
4. | Remove the weather strip and the cowl top cover (A) after removing retainers.
5. | Disconnect the wiper motor connector (A) from the wiper motor & linkage assembly.
6. | Remove the windshield wiper motor and linkage assembly (A) after removing 3 bolts.
7. | Hold the wiper motor crank arm and remove the upper linkage (A) from the wiper motor crank arm.
Before remove the wiper motor and linkage assembly, make sure that the linkage is stopped at automatic stop position. To install the wiper motor crank arm exactly, check that the linkage is aligned with the crank arm in straight line and the angle of each linkages. Put the matchmark on the wiper motor and linkage assembly. Be careful not to bend the linkage.
8. | Remove the lower linkage (A) from the wiper motor crank arm.
To install the wiper motor crank arm exactly, check that the linkage is aligned with the crank arm in straight line and the angle of each linkages. Be careful not to bend the linkage.
9. | Remove the crank arm (A) after loosening a nut (B).
10. | Remove the wiper motor after loosening the 3 screws.
Installation
Do not allow the wiper arm to fall against the windshield, since it may chip or crack the windshield.
1. | Install the wiper motor.
2. | Install the crank arm.
Torque : 12.7-17.6Nm (1.3-1.8, kgf.m, 9.4-13.0 lbf.ft)
To install the wiper motor crank arm, make sure that the linkage is aligned with the crank arm in straight line and set the angle of each linkages exactly using match mark.
3. | Install the lower and upper linkage to the wiper motor crank arm.
To install the wiper motor crank arm, make sure that the linkage is aligned with the crank arm in straight line and set the angle of each linkages exactly. Be careful not to bend the linkage.
4. | Install the wiper motor and linkage assembly and then connect the wiper motor connector.
Torque : 7-11Nm (0.7-1.1, kgf.m, 5.0-7.9 lbf.ft)
5. | Install the cowl top cover.
6. | Install the windshield wiper arm and blade.
Torque : 22.5~26.4 Nm (2.3~2.7 kgf.m, 16.6~21.7 lbf.ft)
- | The windshield wiper motor must be cycled to make sure that it is in the park position. If necessary, adjust the wiper arm and blade.
7. | Install the wiper arm and blade to the specified position (A).
8. | Set the cowl top cover on the specified spray position.
Specified position | Distance (in) | Distance (mm)
A | 18.2 | 577
B | 0.9 | 2
C | 23.5 | 588.5
D | 23.4 | 654
Inspection
Speed Operation Check
1. | Remove the connector (A) from the wiper motor.
No | Description | No | Description
1 | Low | 4 | GND
2 | High | 5 | P (Parking)
3 | Battery (+) | 6 | -
2. | Attach the positive (+) lead from the battery to terminal 3 and the negative (-) lead to terminal 4.
3. | Check that the motor operates at low or high speed as below table.
Common sources of contamination are insects, tree sap, and hot wax treatments used by some commercial car washes. If the blades are not wiping properly, clean both the window and the blades with a good cleaner or mild detergent, and rinse thotoughlly with clean water.