| TUCSON(LM) >2013 > G 2.0 DOHC > Body (Interior and Exterior) > Exterior > Fender>Repair procedures |

Replacement
• | When removing and installing the hood, an assistant is necessary.
• | Be careful not to damage the hood and body.
• | When removing the clips, use a clip remover.
1. | Remove the front bumper. (Refer to the BD group – “Front Bunper” )
2. | Loosen the mud guard mounting screws.
3. | After loosening the mounting screws and clips, then remove the side sill garnish (A).
4. | After loosening the mounting screws, then remove the front bumper side mounting bracket (A).
5. | Using a screwdriver, remove the fender side cover (B).
6. | After loosening the mounting bolts, then remove the fender (A).
7. | Installation is the reverse of removal