| TUCSON(LM) >2013 > G 2.0 DOHC > Suspension System > Front Suspension System > Front Lower Arm>Repair procedures |

Replacement
1. | Remove the front wheel & tire.
Tightening torque : 88.3 ~ 07.9N.m(9.0 ~ 11.0Kgf.m, 65.1 ~ 79.6lb-ft)
Be careful not to damage to the hub bolts when removing the front wheel & tire.Loosen the bolt & nut and then remove the lower arm(A).
2. | Loosen the bolt & nut and then remove the lower arm(A).
Tightening torque : 98.1 ~ 117.7N.m(10.0 ~ 12.0Kgf.m, 72.3 ~ 86.6lb-ft)
3. | Remove the front lower arm(A) and than loosen the bolts & nuts.
Tightening torque : Fornt 98.1 ~ 117.7N.m(10.0 ~ 12.0Kgf.m, 72.3 ~ 86.6lb-ft) Rear 137.3 ~ 156.9N.m(14.0 ~ 16.0Kgf.m, 101.3 ~ 115.7lb-ft)
4. | Installation is the reverse of removal.
Inspection
1. | Check the bushing for wear and deterioration.
2. | Check the lower arm for bending or breakage.
3. | Check the lower arm for deformation.
4. | Check the all bolts and nuts.