| TUCSON(LM) >2013 > G 2.0 DOHC > Fuel System > Fuel Delivery System > Filler-Neck Assembly>Repair procedures |

Removal
1. | Remove the rear-LH wheel, tire, and the inner wheel house.
2. | Disconnect the fuel filler hose (A) and the ventilation hose (B).
3. | Open the fuel filler door and unfasten the filler-neck assembly mounting screw (A).
4. | Remove the filler-neck assembly from the vehicle after removing the bracket mounting nut (A).
Installation
1. | Installation is reverse of removal.
Filler-neck assembly bracket installation nut : 3.9 ~ 5.9 N.m (0.4 ~ 0.6 kgf.m, 2.9 ~ 4.3 lb-ft)