| TUCSON(LM) >2013 > G 2.0 DOHC > Clutch System > General Information>Specifications |

Specifications
Items | Specifications
Engin.e type | θ 2.0
Clutch operation method | Hydraulic type
Clutch disc Type | Single dry with diaphragm
Faling diameter(Outer × inner) | 235 × 155mm(9.2520 × 6.1024 in.)
Clutch cover assembly Type | Diaphragm spring strap
Clutch release cylinder inner diameter | 20.64mm(0.8126 in.)
Clutch master cylinder inner diameter | 15.87mm(0.6248 in.)
Service Standard
Standard value Clutch disc thickness [When free] Distance between inner pad and clutch pedal Clutch pedal free play Clutch pedal stroke Clutch pedal height | 8.0~8.6 mm (0.3150~0.3386 in.) 167 mm (6.5748 in.) 6~13 mm (0.2362~0.5118 in.) 147~153 mm (5.7874~6.0236 in.) 167 mm (6.5748 in.)
Limit Clutch disc rivet sink Diaphragm spring end height difference Clutch replease cylinder clearance to piston Clutch master cylinder clearance to piston | 0.3 mm (0.0118 in.) 0.5 mm (0.0197 in.) 0.15 mm (0.0059 in.) 0.15 mm (0.0059 in.)
Tightening Torques
Item | N.m | kgf.m | lb-ft
Clutch tube to clutch oil regulator | 13 ~ 17 | 1.3 ~ 1.7 | 9.6 ~ 12.5
Clutch tube to clutch hose | 13 ~ 17 | 1.3 ~ 1.7 | 9.6 ~ 12.5
Clutch release cylinder to clutch hose | 25 ~ 35 | 2.5 ~ 3.5 | 18.4 ~ 25.8
Clutch release cylinder bleeder screw | 12 ~ 20 | 1.2 ~ 2.0 | 8.9 ~ 14.5
Clutch cover | 25 ~ 36 | 2.5 ~ 3.6 | 18 ~ 26
Ignition lock switch | 8 ~ 10 | 0.8 ~ 1.0 | 5.9 ~ 7.4
Clutch pedal mounting | 16.7 ~ 25.5 | 1.7 ~ 2.6 | 12.3 ~ 18.8
Lubricants
Items | Specified lubricants | Quantity
Contact surface of release bearing and fulcrum of clutch release fork | CASMOLY L 9508 | 0.3~0.5g
Inner surface of clutch release cylinder and outer circumference of piston and cup | Brake fluid DOT 3 or DOT 4 | As required
Inner surface of clutch disc spline | CASMOLY L 9508 | 0.2g
Inner surface of clutch master cylinder and outer circumference of piston assembly | Brake fluid DOT 3 or DOT 4 | As required
Clutch master cylinder push rod, clevis pin and washer | Wheel bearing grease SAE J310, NLGI No.2 | As required
Clutch pedal shaft and bushings | Chassis grease SAE J310a, NLGI No.1 | As required
Contact portion of release fork to release cylinder push rod | CASMOLY L 9508 | As required