| TUCSON(LM) >2013 > G 2.0 DOHC > Engine Electrical System > Starting System > Starter Relay>Repair procedures |

Inspection
1. | Remove the fuse box cover.
2. | Remove the starter relay (A).
3. | Using an ohmmeter, check that there is continuity between each terminal.
Terminal | Continuity
30 - 87 | NO
85 - 86 | YES
4. | Apply 12V to terminal 85 and ground to terminal 86. Check for continuity between terminals 30 and 87.
5. | If there is no continuity, replace the starter relay.
6. | Install the starter relay.
7. | Install the fuse box cover.