| TUCSON(LM) >2013 > G 2.0 DOHC > Engine Mechanical System > Cylinder Block > Cylinder Block>Repair procedures |

Disassembly
1. | M/T : remove flywheel.
2. | A/T : remove drive plate.
3. | Attach the engine to an engine stand for disassembly.
4. | Remove timing chain. (Refer to Timing system in this group)
5. | Remove cylinder head. (Refer to Cylinder block in this group)
6. | Remove the oil dip stick (A).
7. | Remove knock sensor(A).
8. | Remove oil pressure sensor(A).
9. | Remove the sensor cover and the CKP sensor(A).
10. | Remove water pump.
11. | Remove balance shaft module (oil pump).
12. | Remove ladder frame(A).
13. | Check the connecting rod end play.
14. | Remove the connecting rod caps and check oil clearance.
15. | Remove piston and connecting rod assemblies.
(1) | Using a ridge reamer, remove all the carbon from the top of the cylinder.
(2) | Push the piston, connecting rod assembly and upper bearing through the top of the cylinder block.
• | Keep the bearings, connecting rod and cap together.
• | Arrange the piston and connecting rod assemblies in the correct order.
16. | Remove crankshaft bearing cap and check oil clearance.
17. | Check the crankshaft end play.
18. | Lift the crankshaft(A) out of the engine, being careful not to damage journals.
Arrange the main bearings and thrust bearings in the correct order.
19. | Check fit between piston and piston pin. Try to move the piston back and forth on the piston pin. If any movement is felt, replace the piston and pin as a set.
20. | Remove piston rings.
(1) | Using a piston ring expender, remove the 2 compression rings.
(2) | Remove 2 side rails and the spacer by hand.
Arrange the piston rings in the correct order only.
21. | Disconnect connecting rod from piston.
Inspection
Connecting Rod And Crankshaft
1. | Check the connecting rod end play. Using a feeler gauge, measure the end play while moving the connecting rod back and forth.
Standard end play : 0.1~ 0.25mm(0.004 ~ 0.010in.) Maximum end play : 0.35mm(0.0138in.)
A. | If out-of-tolerance, install a new connecting rod.
B. | If still out-of-tolerance, replace the crankshaft.
2. | Check the connecting road bearing oil clearance.
(1) | Check the matchmarks on the connecting rod and cap are aligned to ensure correct reassembly.
(2) | Remove 2 connecting rod cap bolts.
(3) | Remove the connecting rod cap and bearing half.
(4) | Clean the crank pin and bearing.
(5) | Place plastigage across the crank pin.
(6) | Reinstall the bearing half and cap, and torque the bolts.
Tightening torque 17.7~21.6Nm (1.8~2.2kgf.m, 13.0~15.9lb-ft) + 88~92°
Do not turn the crankshaft.
(7) | Remove 2 bolts, connecting rod cap and bearing half.
(8) | Measure the plastigage at its widest point.
Standard oil clearance 0.031 ~ 0.045mm (0.0012 ~ 0.0017in.)
(9) | If the plastigage measures too wide or too narrow, remove the upper half of the bearing, install a new, complete bearing with the same color mark (select the color as shown in the next column), and recheck the clearance.
Do not file, shim, or scrape the bearings or the caps to adjust clearance.
(10) | If the plastigage shows the clearance is still incorrect, try the next larger or smaller bearing (the color listed above or below that one), and check clearance again.
If the proper clearance cannot be obtained by using the appropriate larger or smaller bearings, replace the crankshaft and start over.
If the marks are indecipherable because of an accumulation of dirt and dust, do not scrub them with a wire brush or scraper. Clean them only with solvent or detergent.
Connecting Rod Mark Location Discrimination Of Connecting Rod
Class | Mark | Inside Diameter
a | A | 51.000 ~ 51.006mm (2.0079 ~ 2.0081in.)
b | B | 51.006 ~ 51.012mm (2.0081 ~ 2.0083in.)
c | C | 51.012 ~ 51.018mm (2.0083 ~ 2.0085in.)
Crankshaft Pin Mark Location Discrimination Of Crankshaft
Conform to read stamping order as shown arrow direction from #1.
Discrimination Of Crankshaft
Class | Mark | Outside Diameter Of Pin
I | 1 | 47.966 ~ 47.972mm (1.8884 ~ 1.8886in.)
II | 2 | 47.960 ~ 47.966mm (1.8881 ~ 1.8884in.)
III | 3 | 47.954 ~ 47.960mm (1.8879 ~ 1.8881in.)
Place Of Identification Mark (Connecting Rod Bearing) Discrimination Of Connecting Rod Bearing Discrimination Of Connecting Rod Bearing
Class | Mark | Thickness Of Bearing
AA | Blue | 1.515 ~ 1.518mm (0.0596 ~ 0.0597in.)
A | Black | 1.512 ~ 1.515mm (0.0595 ~ 0.0596in.)
B | None | 1.509 ~ 1.512mm (0.0594 ~ 0.0595in.)
C | Green | 1.506 ~ 1.509mm (0.0592 ~ 0.0594in.)
D | Yellow | 1.503 ~ 1.506mm (0.0591 ~ 0.0592in.)
(11) | Selection
Crankshaft Indentification Mark | Connecting Rod Identification Mark | Assembing Classification Of Bearing
I (1) | a (A) | D (Yellow)
b (B) | C (Green)
c (C) | B (None)
II (2) | a (A) | C (Green)
b (B) | B (None)
c (C) | A (Black)
III (3) | a (A) | B (None)
b (B) | A (Black)
c (C) | AA (Blue)
3. | Check the crankshaft bearing oil clearance.
(1) | To check main bearing-to-journal oil clearance, remove the main caps and bearing halves.
(2) | Clean each main journal and bearing half with a clean shop tower.
(3) | Place one strip of plastigage across each main journal.
(4) | Reinstall the bearings and caps, then torque the bolts.
Tightening torque 14.7Nm (1.5kgf.m, 10.8lb-ft) + 27.5~31.4Nm (2.8~3.2kgf.m, 20.3~23.1lb-ft) + 120~125°
Do not turn the crankshaft.
(5) | Remove the cap and bearing again, and measure the widest part of the plastigage.
Standard oil clearance 0.020 ~ 0.038mm (0.0008 ~ 0.0015in.)
(6) | If the plastigage measures too wide or too narrow, remove the upper half of the bearing, install a new, complete bearing with the same color mark (select the color as shown in the next column), and recheck the clearance.
Do not file, shim, or scrape the bearings or the caps to adjust clearance.
(7) | If the plastigage shows the clearance is still incorrect, try the next larger or smaller bearing (the color listed above or below that one), and check clearance again.
If the proper clearance cannot be obtained by using the appropriate larger or smaller bearings, replace the crankshaft and start over.
If the marks are indecipherable because of an accumulation of dirt and dust, do not scrub them with a wire brush or scraper. Clean them only with solvent or detergent.
Connecting Rods
1. | When reinstalling, make sure that cylinder numbers put on the connecting rod and cap at disassembly match. When a new connecting rod is installed, make sure that the notches for holding the bearing in place are on the same side.
2. | Replace the connecting rod if it is damaged on the thrust faces at either end. Also if step wear or a severely rough surface of the inside diameter of the small end is apparent, the rod must be replaced as well.
3. | Using a connecting rod aligning tool, check the rod for bend and twist. If the measured value is close to the repair limit, correct the rod by a press. Any connecting rod that has been severely bent or distorted should be replaced.
Allowable bend of connecting rod : 0.05mm / 100mm (0.0020 in./3.94 in.) or less Allowable twist of connecting rod : 0.1mm / 100mm (0.0039 in./3.94 in.) or less
Crankshaft bore mark location Letters have been stamped on the block as a mark for the size of each of the 5 main journal bores. Use them, and the numbers or bar stamped on the crank (marks for main journal size), to choose the correct bearings. Discrimination Of Cylinder Block
Calss | Mark | Inside Diameter
a | A | 56.000 ~ 56.006mm (2.2047 ~ 2.2049in.)
b | B | 56.006 ~ 56.012mm (2.2049 ~ 2.2052in.)
c | C | 56.012 ~ 56.018mm (2.2052 ~ 2.2054in.)
Crankshaft Journal Mark Location Discrimination Of Crankshaft
Conform to read stamping order as shown arrow direction from #1.
Discrimination Of Crankshaft
Class | Mark | Outside Diameter Of Journal
I | 1 | 51.954 ~ 51.960mm (2.0454 ~ 2.0456in.)
II | 2 | 51.948 ~ 51.954mm (2.0452 ~ 2.0454.)
III | 3 | 51.942 ~ 51.948mm (2.0449 ~ 2.0452in.)
Place Of Identification Mark (Crankshaft Bearing) Discrimination Of Crankshaft Bearing Discrimination Of Crankshaft Bearing
Class | Mark | Thickness Of Bearing
AA | Blue | 2.026 ~ 2.029mm (0.0797 ~ 0.0798in.)
A | Black | 2.023 ~ 2.026mm (0.0796 ~ 0.0797in.)
B | None | 2.020 ~ 2.023mm (0.0795 ~ 0.0796in.)
C | Green | 2.017 ~ 2.020mm (0.0794 ~ 0.795in.)
D | Yellow | 2.014 ~ 2.017mm (0.0793 ~ 0.0794in.)
Selection
Crankshaft Identification Mark | Crankshaft Bore Identification Mark | Assembling Classification Of Bearing
I (1) | a (A) | D (Yellow)
b (B) | C (Green)
c (C) | B (None)
II (2) | a (A) | C (Green)
b (B) | B (None)
c (C) | A (Black)
III (3) | a (A) | B (None)
b (B) | A (Black)
c (C) | AA (Blue)
4. | Check crankshaft end play. Using a dial indicator, measure the thrust clearance while prying the crankshaft back and forth with a screwdriver.
Standard end play 0.07 ~ 0.25mm (0.0027 ~ 0.0098in.) Limit : 0.30mm (0.0118in.)
If the end play is greater than maximum, replace the thrust bearings as a set.
Thrust bearing thickness 1.925 ~ 1.965mm(0.0758 ~ 0.07736in.)
5. | Inspect main journals and crank pins Using a micrometer, measure the diameter of each main journal and crank pin.
Main journal diameter : 51.942 ~ 51.960mm (2.0449 ~ 2.0456in.) Crank pin diameter : 47.954 ~ 47.972mm (1.8879 ~ 1.8886in.)
Cylinder Block
1. | Remove gasket material. Using a gasket scraper, remove all the gasket material from the top surface of the cylinder block.
2. | Clean cylinder block Using a soft brush and solvent, thoroughly clean the cylinder block.
3. | Inspect top surface of cylinder block for flatness. Using a precision straight edge and feeler gauge, measure the surface contacting the cylinder head gasket for warpage.
Flatness of cylinder block gasket surface Standard : Less than 0.05mm(0.0020 in.)
4. | Inspect cylinder bore diameter Visually check the cylinder for vertical scratchs. If deep scratches are present, replace the cylinder block.
5. | Inspect cylinder bore diameter Using a cylinder bore gauge, measure the cylinder bore diameter at position in the thrust and axial directions.
Standard diameter [2.4] : 88.00 ~ 88.03mm (3.4645 ~ 3.4657in.) [2.0] : 86.00 ~ 86.03mm (3.3858 ~ 3.3870in.)
Measure position(from the bottom of the cylinder block) : 110.7mm(4.3582in.)/160mm(6.2992in.)/210mm(8.2677in.)
6. | Check the cylinder bore size code on the cylinder block. Cylinder Bore Inner Diameter
Size Code | 2.0 | 2.4
A | 86.00 ~ 86.01mm (3.3858~ 3.3862in.) | 88.00 ~ 88.01mm (3.4645~ 3.4649in.)
B | 86.01 ~ 86.02mm (3.3862~ 3.3866in.) | 88.01 ~ 88.02mm (3.4649~ 3.4653in.)
C | 86.02 ~ 86.03mm (3.3866~ 3.3870in.) | 88.02 ~ 88.03mm (3.4653~ 3.4657in.)
7. | Check the piston size code on the piston top face.
Stamp the grade mark of basic diameter with rubber stamp.
Piston Outer Diameter
Size Code | 2.0 | 2.4
A | 85.975 ~ 85.985mm (3.3848~ 3.3852in.) | 87.975 ~ 87.985mm (3.4635~ 3.4639in.)
B | 85.985 ~85.995mm (3.3852~ 3.3856in.) | 87.985 ~ 87.995mm (3.4639~ 3.4643in.)
C | 85.995 ~ 86.005mm (3.3856~ 3.3860in.) | 87.995 ~88.005mm (3.4643~ 3.4647in.)
8. | Select the piston related to cylinder bore class.
Clearance : 0.015 ~ 0.035mm (0.00059 ~ 0.00137in.)
Piston And Rings
1. | Clean piston
(1) | Using a gasket scraper, remove the carbon from the piston top.
(2) | Using a groove cleaning tool or broken ring, clean the piston ring grooves.
(3) | Using solvent and a brush, thoroughly clean the piston.
Do not use a wire brush.
2. | The standard measurement of the piston outside diameter is taken 34.5 mm (1.35 in.) from the top land of the piston.
Standard diameter [2.4] : 87.975 ~ 88.005mm (3.4635 ~ 3.4647in.) [2.0] : 85.975 ~ 86.005mm (3.3848 ~ 3.3860in.)
3. | Calculate the difference between the cylinder bore diameter and the piston diameter.
Piston-to-cylinder clearance 0.015 ~ 0.035mm(0.00059 ~ 0.00137in.)
4. | Inspect the piston ring side clearance. Using a feeler gauge, measure the clearance between new piston ring and the wall of the ring groove.
Piston ring side clearance Standard No.1 : 0.05 ~ 0.08mm (0.0019 ~ 0.0031in.) No.2 : 0.04 ~ 0.08mm (0.0015 ~ 0.0031in.) Oil ring : 0.06 ~ 0.15mm (0.0023 ~ 0.0059in.) Limit No.1 : 0.1mm (0.004in.) No.2 : 0.1mm (0.004in.) Oil ring : 0.2mm (0.008in.)
If the clearance is greater than maximum, replace the piston.
5. | Inspect piston ring end gap. To measure the piston ring end gap, insert a piston ring into the cylinder bore. Position the ring at right angles to the cylinder wall by gently pressing it down with a piston. Measure the gap with a feeler gauge. If the gap exceeds the service limit, replace the piston ring. If the gap is too large, recheck the cylinder bore diameter against the wear limits, If the bore is over the service limit, the cylinder block must be rebored.
Piston ring end gap Standard No.1 : 0.15 ~ 0.30mm (0.0059 ~ 0.0118in.) No.2 : 0.37 ~ 0.52m (0.0145 ~ 0.0204in.) Oil ring : 0.20 ~ 0.70mm (0.0079 ~ 0.0275in.) Limit No.1 : 0.6mm (0.0236in.) No.2 : 0.7mm (0.0275in.) Oil ring : 0.8mm (0.0315in.)
Piston Pins
1. | Measure the diameter of the piston pin.
Piston pin diameter 21.001 ~ 21.006mm (0.8268 ~ 0.8270in.)
2. | Measure the piston pin-to-piston clearance.
Piston pin-to-piston clearance 0.013 ~ 0.023mm (0.0005 ~ 0.0009in.)
3. | Check the difference between the piston pin diameter and the connecting rod small end diameter.
Piston pin-to-connecting rod interference 0.016 ~ 0.032mm (0.00063 ~ 0.00126in.)
Reassembly
• | Thoroughly clean all parts to assembled.
• | Before installing the parts, apply fresh engine oil to all sliding and rotating surfaces.
• | Replace all gaskets, O-rings and oil seals with new parts.
1. | Assemble piston and connecting rod.
(1) | Before pressing the piston pin, apply a coat of lubricant oil to the piston pin outer and connecting rod.
• | Take care that piston pin is not to be damaged during pressing process.
• | When replace the piston pin, check the piston pin outer diameter and connecting rod small end inner diameter as below.
Piston pin outer DIA. : 21.001 ~ 21.006mm (0.8268 ~ 0.8270in) Connecting rod small end inner DIA. : 20.974 ~ 20.985mm (0.8257 ~ 0.8261in) Interference: -0.032 ~ -0.016 mm (-0.0013 ~ -0.0006 in.)
(2) | Use a hydraulic press for installation.
(3) | The piston front mark and the connecting rod front mark must face the timing belt side of the engine.
2. | Install piston rings.
(1) | Install the oil ring spacer and 2 side rails by hand.
(2) | Using a piston ring expander, install the 2 compression rings with the code mark facing upward.
(3) | Position the piston rings so that the ring ends are as shown.
3. | Install connecting rod bearings.
(1) | Align the bearing claw with the groove of the connecting rod or connecting rod cap.
(2) | Install the bearings(A) in the connecting rod and connecting rod cap(B).
4. | Install main bearings.
Upper bearings have an oil groove of oil holes; Lower bearings do not.
(1) | Align the bearing claw with the claw groove of the cylinder block, push in the 5 upper bearings(A).
(2) | Align the bearing claw with the claw groove of the main bearing cap, and push in the 5 lower bearings.
5. | Install thrust bearings. Install the 2 thrust bearings(A) under the No.3 journal position of the cylinder block with the oil grooves facing outward.
6. | Place crankshaft(A) on the cylinder block.
7. | Place main bearing caps on cylinder block.
8. | Install main bearing cap bolts.
Always use new main bearing cap bolts.
• | The main bearing cap bolts are tightened in 2 progressive steps.
• | If any of the bearing cap bolts in broken or deformed, replace it.
(1) | Apply a light coat of engine oil on the threads and under the bearing cap bolts.
(2) | Install and uniformly tighten the 10 bearing cap bolts(A), in several passes, in the sequence shown.
Tightening torque 14.7Nm (1.5kgf.m, 10.8lb-ft) + 27.5~31.4Nm (2.8~3.2kgf.m, 20.3~23.1lb-ft) + 120~125°
(3) | Check that the crankshaft turns smoothly.
9. | Check crankshaft end play.
10. | Install piston and connecting rod assemblies.
Before installing the pistons, apply a coat of engine oil to the ring grooves and cylinder bores.
(1) | Remove the connecting rod caps, and slip short sections of rubber hose over the threaded ends of the connecting rod bolts.
(2) | Install the ring compressor, check that the bearing is securely in place, then position the piston in the cylinder, and tap it in using the wooden handle of a hammer.
(3) | Stop after the ring compressor pops free, and check the connecting rod-to-check journal alignment before pushing the piston into place.
(4) | Apply engine oil to the bolt threads. Install the rod caps with bearings, and torque the bolts.
Tightening torque 17.7~21.6Nm (1.8~2.2kgf.m, 13.0~15.9lb-ft) + 88~92°
Always use new connecting rod cap bolts.
Maintain downward force on the ring compressor to prevent the rings from expanding before entering the cylinder bore.
11. | Apply liquid gasket to the mating surface of cylinder block and ladder frame.
• | Be assembling ladder frame, the liquid sealant Loctite 5900 or THREEBOND 1217H should be applied ladder frame.
• | The part must be assembled within 5 minutes after sealant was applied.
• | Apply sealant to the inner threads of the bolt holes.
12. | Install ladder frame(A) with 10 bolts in several passes in sequence shown.
Tightening torque Step 1 : 8.8 ~ 9.8N.m (0.9 ~ 1.0kgf.m, 6.5 ~ 7.2lb-ft) Step 2 : 17.7 ~20.6N.m (1.8 ~ 2.1kgf.m, 3.0 ~ 15.2lb-ft) Step 3 : 27.5 ~ 31.4N.m (2.8 ~ 3.2kgf.m, 20.3 ~ 23.1lb-ft)
13. | Install rear oil seal.
(1) | Apply engine oil to a new oil seal lip.
(2) | Using SST(09231-H1100, 09214-3K100) and a hammer, tap in the oil seal until its surface is flush with the rear oil seal retainer edge.
14. | Install balance shaft module (oil pump).
15. | Install water pump.
16. | Install CKP sensor(A) and sensor cover.
Tightening torque 9.8 ~ 11.8N.m (1.0 ~ 1.2kgf.m, 7.2 ~ 8.7lb-ft)
17. | Install oil pressure sensor.
(1) | Apply adhesive to 2 or 3 threads. Adhesive : MS 721-39(B) or equivalent.
(2) | Install the oil pressure sensor (A).
Tightening torque 7.8 ~ 11.8N.m (0.8 ~ 1.2kgf.m, 5.8 ~ 8.7lb-ft)
18. | Install knock sensor(A).
Tightening torque 18.6 ~ 23.5N.m (1.9 ~ 2.4kgf.m, 13.7 ~ 17.4lb-ft)
19. | Install oil level gauge assembly.
(1) | Install a new O-ring on the oil dip stick.
(2) | Apply engine oil on the O-ring.
(3) | Install the oil dip stick (A) with the bolt.
Tightening torque 7.8 ~ 11.8N.m (0.8 ~ 1.2kgf.m, 5.8 ~ 8.7lb-ft)
20. | Install the cylinder head. (Refer to Cylinder head assembly in this group)
21. | Install the timing chain. (Refer to Timing system in this group)
22. | Install the oil pan.
(1) | Using a razor blade and gasket scraper, remove all the old gasket material from the gasket surfaces.
Check that the mating surfaces are clean and dry before applying liquid gasket.
(2) | Apply liquid gasket as an even bead, centered between the edges of the mating surface. Use liquid gasket LOCTITE5900H or THREEBOND 1217H or equivalent(MS721-40).
Bead width : 3.0mm (0.12in)
• | To prevent leakage of oil, apply liquid gasket to the inner threads of the bolt holes.
• | Do not install the parts if five minutes or more have elapsed since applying the liquid gasket. Instead, reapply liquid gasket after removing the residue.
• | After assembly, wait at least 30 minutes before filling the engine with oil.
(3) | Install the oil pan(A). Uniformly tighten the bolts in several passes.
Tightening torque M9(B):30.4 ~ 34.3N.m (3.1 ~ 3.5kgf.m, 22.4 ~ 25.3lb-ft) M6(C):9.8 ~ 11.8N.m (1.0 ~ 1.2kgf.m, 7.2 ~ 8.7lb-ft)
23. | Remove engine stand.
24. | A/T : Install drive plate(A).
Tightening torque 117.7 ~ 127.5N.m (12 ~ 13kgf.m, 86.8 ~ 94.0lb-ft)
M/T : Install flywheel(B).
Tightening torque 117.7 ~ 127.5N.m (12 ~ 13kgf.m, 86.8 ~ 94.0lb-ft)
• | Always use new flywheel(drive plate) bolts(C).
• | Apply sealant to the screw part(8mm from the end of the bolt) when using new flywheel bolts.
Sealant : Three bond 2403, Loctite 200 or 204
• | Install and uniformly tighten the 7 bolts, in several passes.