| TUCSON(LM) >2013 > G 2.4 DOHC > Body Electrical System > Power Windows > Power Window Switch>Repair procedures |

Inspection
Main Power Window Switch Inspection
1. | Disconnect the negative (-) battery terminal.
2. | Remove the front door trim and power window switch. (Refer to the BD group - "Front door")
3. | Check for continuity between the terminals in each switch position according to the table. If the continuity condition is not normal, replace the switch. [Driver Auto Up/Down]
Passenger Power Window Switch Inspection
1. | Disconnect the negative (-) battery terminal.
2. | Remove the front door trim and power window switch. (Refer to the BD group - "Front door")
3. | Check for continuity between the terminals in each switch position according to the table. If the continuity condition is not normal, replace the switch. [Power Door Lock] [General]
Rear Power Window Switch Inspection
1. | Disconnect the negative (-) battery terminal.
2. | Remove the rear door trim. (Refer to the BD group - "Rear door")
3. | Remove the rear power window switch module (A).
4. | Check for continuity between the terminals in each switch position according to the table. If the continuity condition is not normal, replace the switch. [General]