| TUCSON(LM) >2013 > G 2.4 DOHC > Body Electrical System > Ignition Switch Assembly>Repair procedures |

Inspection
1. | Disconnect the ignition switch connector (B) and key warning switch connector (A) from under the steering column.
2. | Check for continuity between the terminals.
3. | If continuity is not specified, replace the switch.
Removal
1. | Disconnect the negative (-) battery terminal.
2. | Remove the steering column upper and lower shrouds. (Refer to the ST group - "Steering column")
3. | Remove the ignition switch (A) after disconnecting the 6P connector (B).
4. | Remove the key warning and immobilizer connector (A).
5. | Remove the key illumination lens (A).
6. | If it is necessary to remove the key lock cylinder (A), remove the key lock cylinder after pushing lock pin (B) with key ACC.
Installation
1. | Install the key lock cylinder.
2. | Install the illumination bulb, lens and cover.
3. | Install the key warning and immobilizer connector.
4. | Install the ignition switch.
5. | Install the steering column shrouds and crash pad lower panel.