| TUCSON(LM) >2013 > G 2.4 DOHC > Body Electrical System > Panoramaroof > Panoramaroof Motor>Repair procedures |

Replacement
1. | Disconnect the negative (-) battery terminal.
2. | Remove the roof trim. (Refer to the BD group - "Roof trim")
3. | Remove the panoramaroof motor (A) after disconnecting the connector (10 Pin).
4. | Ground the terminals as below table, and check that the panoramaroof unit operates as below table.
5. | Make these input tests at the motor connector of panoramaroof harness if any test indicates a problem, find and correct the cause, then recheck the system. If all the input tests prove OK, the sunroof motor must be faulty; replace it.
Terminal | Test condition | Test : Desired result
3 | IG2 ON | Check for voltage to ground : There should be battery voltage
1 | Under all conditions | Check for continuity to ground : There should be continuity.
6 | Under all conditions | Check for voltage to ground : There should be battery voltage.
6. | Make these input tests at the console connector of panoramaroof harness if any test indicates a problem, find and correct the cause, then recheck the system. If all the input tests prove OK, the sunroof motor must be faulty; replace it.
Terminal | Test condition | Test : Desired result
3 | IG2 ON | Check for voltage to ground :
There should be battery voltage
1 | Under all conditions | Check for continuity to ground :
There should be continuity.
2 | Under all conditions | Check for voltage to ground :
There should be battery voltage.
Resetting The Panoramaroof Whenever the vehicle battery is disconnected or discharged, or you use the emergency handle to operate the Panoramaroof, you have to reset your Panoramaroof system as follows :
1. | Turn the ignition key to the ON position and then close the panoramaroof completely.
2. | Release the panoramaroof control lever.
3. | Press and hold the CLOSE button for more than 10 seconds until the sunroof has moved slightly.
4. | Release the panoramaroof control lever.
5. | Press and hold the CLOSE button once again until the sunroof do as follows;
A. | Tilt → Slide Open → Slide Close Then release the lever.
6. | Reset procedure of panorama system is finished.
Protecting The Overheated Motor In order to protect the overheated Panoramaroof motor by continuous motor operation, the Panoramaroof ECU controls the Run-time and Cool-time of motor as followings;
1. | The Panoramaroof ECU detects the Run- time of motor
2. | Motor can be operated continuously for the 1st Run-time(120 ± 10sec.).
3. | Motor which is operated continuously stops operating after the 1st Run-time(120 ± 10sec.).
4. | And then Motor is not operated for the 1st Cool-time(18 ± 2sec.).
5. | Motor is operated for the 2nd Run-time(10 ± 2sec.) at the continued motor operation after 1st Cool-time(18 ± 2sec.)
6. | Motor which is operated continuously stops operating after the 2nd Run-time(10 ± 2sec.)
7. | Motor is not operated for the 2nd Cool-time(18 ± 2sec.).
8. | Motor repeats the 2nd Run-time and 2nd Cool-time at the continued motor operation.
A. | In case that motor is not operated continuously, the Run-time which is limited for protecting the overheated motor is increased.
B. | The Run-Time of motor is initialized to "0" if the battery or fuse is reconnected after being disconnected, discharged or blown.
T1 : 120 ± 10 sec., T2 : 18 ± 2 sec., T3 : 10 ± 2 sec., T4 : 18 ± 2 sec.