| TUCSON(LM) >2013 > G 2.4 DOHC > Restraint > Airbag Module > Curtain Airbag (CAB) Module>Repair procedures |

Removal
1. | Disconnect the battery negative cable and wait for at least 3 minutes before beginning work.
2. | Remove the roof trim. (Refer to the Body group- Interior)
3. | Disconnect the curtain airbag harness connector.
4. | After loosening the mounting bolts and nuts remove the curtain airbag.
Installation
1. | Remove the ignition key from the vehicle.
2. | Disconnect the battery negative cable and wait for at least three minutes.
3. | Tighten the curtain airbag mounting bolts.
Tightening torque: 7.0 ~ 9.0 N.m (0.7 ~ 0.9 kgf.m, 5.1 ~ 6.6 lb-ft)
• | Never twist the airbag module when installing it. If the module is twisted, airbag module may operate abnormally.
4. | Connect the curtain airbag connector.
5. | Install the roof trim. (Refer to the Body group- Interior)
6. | Reconnect the battery negative cable.
7. | After installing the curtain airbag (CAB), confirm proper system operation:
A. | Turn the ignition switch ON; the SRS indicator light should be turned on for about six seconds and then go off.