| TUCSON(LM) >2013 > G 2.4 DOHC > Body Electrical System > Lighting System > Rheostat>Repair procedures |

Inspection
1. | Disconnect the negative (-) battery terminal.
2. | Remove the crash pad lower panel. (Refer to the BD group - "Crash pad")
3. | Remove the crash pad side switch assembly (A) as shown below picture.
Put on gloves to protect your hands.
4. | Remove the rheostat switch (A) after disconnecting the connectors.
Take care not to damage the hook when removing the rheostat switch.
5. | Operate the switch and check for continuity between terminals with an ohmmeter.