| VELOSTER(FS) >2012 > G 1.6 GDI > Body (Interior and Exterior) > Seat Belt > Rear Seat Belt>Repair procedures |

Replacement
Rear Seat Belt Replacement
• | When installing the belt, make sure not to damage the retractor.
1. | Remove the following items first :
A. | Rear seat assembly (Refer to the BD group - "Rear Seat")
B. | Front door scuff trim [LH] (Refer to the BD group - "Interior Trim")
C. | Rear door scuff trim [RH] (Refer to the BD group - "Interior Trim")
2. | Using a screwdriver or remover, remove the rear transverse trim (A).
3. | After loosening the mounting bolt, then remove the rear seat belt lower anchor (A). [LH, RH]
Tightening torque : 39.2 ~ 53.9 N.m (4.0 ~ 5.5 kgf.m, 28.9 ~ 39.8 lb-ft)
4. | Using a screwdriver or remover, remove the center pillar lower trim (A). [LH]
5. | Using a screwdriver or remover, remove the luggage side trim lamp (A).
6. | Disconnect the luggage side trim lamp connector (B).
7. | After loosening the mounting screws, then remove the luggage side trim (C). [LH] [RH]
8. | After loosening the mounting bolt, then remove the rear seat belt (A) and rear seat belt retractor (B).
Tightening torque : 39.2 ~ 53.9 N.m (4.0 ~ 5.5 kgf.m, 28.9 ~ 39.8 lb-ft)
9. | Installation is the reverse of removal.
• | Make sure the connector is plugged in properly.
• | Replace any damage clips.
Rear Seat Belt Buckle Replacement
1. | Remove the following items first :
A. | Rear seat cushion assembly (Refer to the BD group - "Rear Seat")
2. | After loosening the mounting bolt, then remove the rear seat belt buckle (A). [LH]
Tightening torque : 39.2 ~ 53.9 N.m (4.0 ~ 5.5 kgf.m, 28.9 ~ 39.8 lb-ft)
[RH]
Tightening torque : 39.2 ~ 53.9 N.m (4.0 ~ 5.5 kgf.m, 28.9 ~ 39.8 lb-ft)
3. | Installation is the reverse of removal.