| VELOSTER(FS) >2012 > G 1.6 GDI > Heating,Ventilation, Air Conditioning > General Information>Specifications |

Specification
Air conditioner
Item | Specification
Compressor | Type | DV 13
Oil type & Capacity | PAG OIL 120±10cc
Displacement | 130cc/rev
Condenser | Heat rejection | 11,900 - 3% kcal/hr
A/C Pressure transducer | The method to measure the pressure | Voltage= 0.00878835 * P + 0.5
Expansion valve | Type | Block type
Refrigerant | Type | R-134a
Capacity [g(oz.)] | 420±25 (14.8±0.88)
Blower unit
Item | Specification
Fresh and recirculation | Operating method | Actuator
Blower | Type | Sirocco
Speed step | 1~4 speed (Manual)
Speed control | Resistor (Manual)
Air filter | Type | Particle filter
Heater and evaporator unit
Item | Specification
Heater | Type | Pin & Tube type
Heating capacity | 4,650 ± 3% kcal/hr
Mode operating method | Actuator
Temperature operating method | Actuator
Evaporator | Temperature control type | Evaporator temperature sensor
A/C ON/OFF [°C(°F)] | ON : 2.5±0.3 (36.5±0.5), OFF: 0.5±0.3 (32.9±0.5)