| VELOSTER(FS) >2012 > G 1.6 GDI > Body (Interior and Exterior) > Body Dimensions>General Information |

General
1. | Basically, all measurements in this manual are taken with a tracking gauge.
2. | When a measuring tape is used, check to be sure there is no elongation, twisting or bending.
3. | For measuring dimensions, both projected dimension and actual-measurement dimension are used in this manual.
Measurement Method
Projected Dimensions
1. | These are the dimensions measured when the measurement points are projected into the reference plane, and are the reference dimensions used for body alterations.
2. | If the length of the tracking gauge probes is adjustable, make the measurement by lengthening one probe by the amount equivalent to the difference in height of the two surfaces.
Actual-Measurement Dimensions
1. | These dimensions indicate the actual linear distance between measurement points, and are the reference dimensions for use if a tracking gauge is used for measurement.
2. | Measure by first adjusting both probes to the same length (A=A').
Check the probes and gauge itself to make sure there is no free play.
Measurement Point
1. | Measurements should be taken at the hole center.