| VELOSTER(FS) >2012 > G 1.6 GDI > Manual Transaxle System > Manual Transaxle Control System > Shift Lever>Repair procedures |

Removal
Shift Lever Assembly Replacement
1. | Remove the floor Interior console assembly. (Refer to "Interior(Console)" in BD group)
2. | Remove the cover (A).
3. | Remove the select cable (B) by removing the snap pin (A).
4. | Remove the shift lever assembly (B) by removing the bolts (A-4ea).
Tightening torque: 9.8 ~ 14.7 N.m (1.0 ~ 1.5 kgf.m, 7.2 ~ 14.5 lb-ft)
5. | Remove the shift cable (B) by removing the clip (A).
6. | Installation is the reverse of removal.
Select / Shift Cable Replacement
1. | Remove the floor Interior console assembly. (Refer to "Interior(Console)" in BD group)
2. | Remove the cover (A).
3. | Remove the select cable (B) by removing the snap pin (A).
4. | Remove the shift lever assembly (B) by removing the bolts (A-4ea).
Tightening torque: 9.8 ~ 14.7 N.m (1.0 ~ 1.5 kgf.m, 7.2 ~ 14.5 lb-ft)
5. | Remove the shift cable (B) by removing the clip (A).
6. | Remove the retainer (A) and nuts (B-2ea).
Tightening torque: 11.8 ~ 14.7 N.m (1.2 ~ 1.5 kgf.m, 8.7 ~ 10.8 lb-ft)
7. | Disconnect the select and shift cable assembly (B) after removing the pin (A).
8. | Remove the shift cable and select cable at cabin room.
9. | Installation is the reverse of removal.
[Shift / Select Cable Installation Tips]
1. | Install the select and shift cable assembly (B) after removing the pin (A).
2. | Install is the shift cable (A).
At this time, have to disconnect select cable.
3. | Install is the shift lever assembly (A).
Tightening torque: 8.8 ~ 13.7 N.m (0.9 ~ 1.4 kgf.m, 6.5 ~ 10.1 lb-ft)
4. | Shift to the 3th gear position.
5. | Insert the selected cable (A) to the shift lever assembly pin (B).
6. | You have to push in the adjuster (C).
7. | Remove the neutral position pin (D).
8. | Install the snap pin (E).
Inspection
1. | Check the select cable for proper operation and for damage.
2. | Check the shift cable for proper operation and for damage.
3. | Check the boots for damage.
4. | Check the boots for wear abrasion sticking, restricted movement or damage.
5. | Check for the weak or damaged spring.
Adjustment
1. | In neutral position, disjoin select cable (A) from shift lever assembly pin (B).
2. | Disconnect select adjuster (A) to an arrow.
3. | Shift to the 3th gear position.
4. | Adjustment adjuster (B) on select cable (A) as rolling from side to side.
5. | Insert on free load and press the adjuster.
6. | After shifting 2nd gear, cheking the left select gap about 1mm(if not, loop no, 1~5)
If there are still gate blocking in spite of re-adjustment, shift lever assembly stopper stoke must be cheked.
7. | In neutral position, join by clip (A).