| VELOSTER(FS) >2012 > G 1.6 GDI > Body Electrical System > Lighting System > Fog Lamps>Repair procedures |

Inspection
1. | Disconnect the negative (-) battery terminal.
2. | Remove the lighting switch of the multifunction switch. (Refer to the "Multifunction Switch")
3. | With the front fog lamp switch, make sure that continuity exists between the terminals below. If continuity is not as specified, replace the multifunction switch.
Fog lamp switch
Removal
1. | Disconnect the negative(-) battery terminal.
2. | Remove the front bumper. (Refer to the BD group - "Front bumper")
3. | Remove the front fog lamp connector(A) from the front bumper.
4. | Remove the front fog bulb(A) turning it in the counterclockwise direction.
5. | Remove the front fog lamp assembly(A).
Installation
1. | Install the front fog bulb.
2. | Reconnect the lamp connector.
3. | Install the front bumper.