| VELOSTER(FS) >2012 > G 1.6 GDI > Heating,Ventilation, Air Conditioning > Blower > Blower Motor>Repair procedures |

Inspection
1. | Connect the battery voltage and check the blower motor rotation.
2. | If the blower motor voltage is not operated well, substitute with a known-good blower motor and check for proper operation.
3. | If the problem is corrected, replace the blower motor.
Replacement
1. | Disconnect the negative (-) battery terminal.
2. | Disconnect the connector (A) of the blower motor.
3. | Remove the blower motor (B) after loosening the mounting screws.
4. | Installation is the reverse order of removal.