| VELOSTER(FS) >2012 > G 1.6 GDI > Manual Transaxle System > General Information>Specifications |

Specifications
Transaxle type | M6CF1
Engine type | Gasoline 1.6 GDI
Gear ratio | 1st | 3.615
2nd | 1.955
3rd | 1.370
4th | 1.036
5th | 0.839
6th | 0.727
Reverse | 3.700
Final gear ratio | 4.267
Tightening Torques
Items | N.m | kgf.m | lb-ft
Oil drain plug | 58.9 ~ 78.5 | 6.0 ~ 8.0 | 43.4 ~ 57.8
Oil filler plug | 58.9 ~ 78.5 | 6.0 ~ 8.0 | 43.4 ~ 57.8
Shift lever assembly bolt | 9.8 ~ 14.7 | 1.0 ~ 1.5 | 7.2 ~ 14.5
Control shaft complete | 19.6 ~ 26.5 | 2.0 ~ 2.7 | 14.4 ~ 19.5
Shift control cable bracket bolt | 14.7 ~ 21.6 | 1.5 ~ 2.2 | 10.9 ~ 15.9
Back up lamp switch | 39.2 ~ 58.9 | 4.0 ~ 6.0 | 28.9 ~ 43.4
Transaxle support bracket bolt | 58.9 ~ 78.5 | 6.0 ~ 8.0 | 43.4 ~ 57.8
Under cover installation bolt | 6.9 ~ 10.8 | 0.7 ~ 1.1 | 5.1 ~ 8.0
Clutch release cylinder installation nut | 14.7 ~ 21.6 | 1.5 ~ 2.2 | 10.9 ~ 15.9
Retainer installation nut | 11.8 ~ 14.7 | 1.2 ~ 1.5 | 8.7 ~ 10.8
Start motor installation bolt | 42.2 ~ 53.9 | 4.3 ~ 5.5 | 31.1 ~ 39.8
Roll rod support bracket bolt | 49.0 ~ 68.6 | 5.0 ~ 7.0 | 36.2 ~ 50.6
107.9 ~ 127.5 | 11.0 ~ 13.0 | 79.6 ~ 94.1
Transaxle upper mounting bolt (TM=>ENG) | 42.2 ~ 53.9 | 4.3 ~ 5.5 | 31.1 ~ 39.8
Transaxle lower mounting bolt (ENG=>TM) | 42.2 ~ 48.1 | 4.3 ~ 4.9 | 31.1 ~ 35.4
42.2 ~ 53.9 | 4.3 ~ 5.5 | 31.1 ~ 39.8
Lubricants and Sealant
Items | Recommnend lubricant | Quantity
Transaxle gear oil | SAE 75W/85 API GL-4 TGO-8 (MS517-14) | 1.8 ~ 1.9L (0.48 ~ 0.50 U.S.gal., 1.90 ~ 2.01 U.S. qt., 1.58 ~ 1.67 lmp qt.)
Transaxle housing | Sealant (MS721-40 or MS721-38) | As requried (Ø1.0 ~ Ø1.5 mm)
Surface of release fork and bearing | Grease (CASMOLY L9508) | As required