| VELOSTER(FS) >2012 > G 1.6 GDI > Body Electrical System > Ignition Switch Assembly>Repair procedures |

Removal
1. | Disconnect the negative (-) battery terminal.
2. | Remove the driver crash pad lower panel. (Refer to the BD group - "Crash pad")
3. | Remove the steering column upper and lower shrouds. (Refer to the BD group - "Crash pad")
4. | Remove the wiper switch. (Refer to the BE group - "Multifunction switch")
5. | Remove the ignition switch after disconnecting the ignition switch 6P connector.
6. | Remove the key warning/immobilizer connector (A).
7. | After loosening the screw, remove the key warning switch (B).
8. | Pushing lock pin with key ACC.
9. | Remove the key lock cylinder (A).
Installation
1. | Install the key lock cylinder.
2. | Install the key warning switch.
3. | Install the key warning/immobilizer connector.
4. | Connect the ignition switch connector after Install the ignition switch.
5. | Install the wiper switch.
6. | Install the steering column shrouds.
7. | Install the driver crash pad lower panel.
Inspection
1. | Disconnect the ignition switch connector (B) and key warning switch connector (A) from the steering column.
2. | Check for continuity between the terminals.
3. | If continuity is not as specified, replace the switch.