| VELOSTER(FS) >2012 > G 1.6 GDI > Heating,Ventilation, Air Conditioning > Air Conditioning System > Ambient Sensor>Description and Operation |

Description
1. | The ambient temperature sensor is located at the front of the condenser and detects ambient air temperature. It is a negative type thermistor; resistance will increase with lower temperature, and decrease with higher temperatures.
2. | The sensor output will be displayed on the AVN.