| VELOSTER(FS) >2012 > G 1.6 GDI > Body (Interior and Exterior) > Body Dimensions > Front Body>Body Repair |

Front Body A
Hood hinge mounting hole (Ø10) | Fender apron upper member corner | Front shock absorber housing cover tooling hole (Ø6.6)
Cowl top cover mounting hole (Ø7) | Side outer panel front corner | Front pillar outer panel corner
Front Body B
Hood hinge mounting hole (Ø10) | Fender apron upper member corner | Cowl top cover mounting hole (Ø7)
Engine mounting bracket hole (Ø12) | Transaxle mounting hole (Ø12) | Engine mounting bracket hole (Ø15)
Transaxle mounting hole (Ø15.5) | Front side member tooling hole (Ø9) | Front side member tooling hole (Ø6.6)
Front end module mounting hole (Ø11.5) | Front end module mounting hole (Ø11.5) |
Front Body C
Engine mounting bracket hole (Ø12) | Transaxle mounting hole (Ø12) | Engine mounting bracket hole (Ø15)
Transaxle mounting hole (Ø15.5) | Front side member tooling hole (Ø9) | Front side member tooling hole (Ø6.6)