| VELOSTER(FS) >2012 > G 1.6 GDI > Body Electrical System > Lighting System > Turn Signal Lamp>Repair procedures |

Removal
Door Mirror Turn Signal Lamp
1. | Disconnect the negative(-) battery terminal.
2. | Remove the mirror(A) from the mirror holder.
Take care not to damage the mirror cover fixing clip.
3. | Loosen the fixing clip and remove the door mirror cover(A).
Take care not to damage the mirror cover fixing clip.
4. | Loosen a screw and disconnect a connector(A). Remove the door mirror turn signal lamp(B).
Installation
Door Mirror Turn Signal Lamp
1. | Install the door mirror turn signal lamp after connecting the connector.
2. | Install the door mirror cover.
3. | Connect the battery terminal (-) and check the lamp operation.