| VELOSTER(FS) >2012 > G 1.6 GDI > Heating,Ventilation, Air Conditioning > Blower > Climate Control Air Filter>Repair procedures |

Replacement
1. | Remove the stopper (A) from the glove box (C) and then disconnect the glove box lift rod (B).
2. | Remove the filter cover (A) with pushing the knob.
3. | Replace the air filter (A) after making sure of the direction of air filter.
In case of driving in an air-polluted area or rugged terrain, check and replace the air filter as frequently as possible.
4. | Installation is the reverse order of removal.