| VELOSTER(FS) >2012 > G 1.6 GDI > Body Electrical System > Power Door Locks > Power Door Lock Switch>Repair procedures |

Inspection
Diagnosis With GDS
1. | It will be able to diagnose defects of power door lock with GDS quickly. GDS can operates actuator forcefully, input/output value monitoring and self diagnosis.
2. | Select model and "BCM".
3. | Select the "SJB" to check.
4. | Select "Current data", if you will check current data of power door lock system. It provides input/output status of SJB.
5. | To check the power door lock operation manually, select "Actuation test".
Removal
1. | Disconnect the negative(-) battery terminal.
2. | Remove the front door trim. (Refer to the BD group - "Front door")
3. | Remove the grip holder cover, after loosening the screw (4EA).
4. | Remove the grip holder cover bracket.
5. | Remover the power window switch (A), after loosening the bolts (4EA).
Installation
1. | Install the power window switch.
2. | Install the grip holder cover.
3. | Connect the connector and install the front door trim panel.