| VELOSTER(FS) >2012 > G 1.6 GDI > Body (Interior and Exterior) > Seat Belt > Front Seat Belt>Repair procedures |

Replacement
Front Seat Belt Replacement
• | When installing the belt, make sure not to damaged the pretensioner.
1. | Remove the following items first :
A. | Front seat assembly (Refer to the BD group - "Front Seat")
B. | Front door scuff trim (Refer to the BD group - "Interior Trim")
C. | Rear door scuff trim [RH] (Refer to the BD group - "Interior Trim")
2. | Disconnect the battery negative cable, and wait for at least three minutes before beginning work.
3. | The seat belt anchor pretensioner (A) be removed after pushing the lock pin (B) as arrow direction. [LH] [RH]
4. | Using a screwdriver or remover, remove the center pillar lower trim (A). [LH] [RH]
5. | Using a screwdriver or remover, remove the front seat belt upper anchor cover (A). [LH] [RH]
6. | After loosening the mounting bolt, then remove the front seat belt upper anchor (A). [LH]
Tightening torque : 39.2 ~ 53.9 N.m (4.0 ~ 5.5 kgf.m, 28.9 ~ 39.8 lb-ft )
[RH]
Tightening torque : 39.2 ~ 53.9 N.m (4.0 ~ 5.5 kgf.m, 28.9 ~ 39.8 lb-ft )
7. | After loosening the mounting bolt, then remove the center pillar upper trim (A). [LH] [RH]
8. | After disconnecting the pretensioner connector lock pin, remove the seat belt pretensioner connector (A), loosen the mounting bolts, then remove the pretensioner (B).
Tightening torque : 39.2 ~ 53.9 N.m (4.0 ~ 5.5 kgf.m, 28.9 ~ 39.8 lb-ft )
9. | Installation is the reverse of removal.
• | Make sure the connector is plugged in properly.
• | Replace any damage clips.
Front Seat Belt Buckle Replacement
1. | Remove the following items first :
A. | Front seat assembly (Refer to the BD group - "Front Seat")
2. | After loosening the mounting screws, then remove the front seat track side cover (A).
3. | Remove the seat belt buckle connector mounting clip (A).
4. | After loosening the mounting bolt, then remove the front seat belt buckle (A).
Tightening torque : 39.2 ~ 53.9 N.m (4.0 ~ 5.5 kgf.m, 28.9 ~ 39.8 lb-ft)
5. | Installation is the reverse of removal.
• | Replace any damage clips.