| VELOSTER(FS) >2012 > G 1.6 GDI > Body Electrical System > Rear Wiper/Washer > Rear Wiper Motor>Repair procedures |

Inspection
Rear Wiper Motor
1. | Remove the connector from the rear wiper motor.
2. | Connect battery positive (+) and negative (-) cables to terminals 3 and 4 respectively.
3. | Check that the motor operates normally. Replace the motor if it operates abnormally.
No | Description | No | Description
1 | Battery | 3 | Switch
2 | Parking | 4 | Ground
Automatic Stop Operation Check
1. | Operate the motor at low speed using the speed control.
2. | Stop the motor operation anywhere except at the off position by disconnecting terminal 3.
3. | Connect terminals 2 and 3.
4. | Connect the positive (+) lead from the battery to terminal 1 and the negative (-) lead to terminal 4.
5. | Check that the motor stops running at the off position.
Removal
1. | Detach the rear wiper head cap (A).
2. | Remove the rear wiper arm & blade (A) after removing rear wiper arm nut (B).
3. | Remove the rear wiper grommet.
4. | Open the tailgate then remove the tailgate trim. (Refer to the BD group - "Tailgate")
5. | Disconnect the rear wiper motor connector (A) then remove the rear wiper motor (B) after loosening bolts (3EA).
Installation
1. | Install the rear wiper motor assembly and the grommet.
Do not reuse the rubber pad if it is damaged.
2. | Install the tailgate trim. (Refer to the BD group - "Tailgate")
3. | Set the rear wiper blade and to the lowest defogger heat line and tailgate glass.
4. | Set the rear washer nozzle on the specified spray position.
5. | Install the rear wiper cap and rear wiper nut.
Tightening torque Nut : 9.8 ~ 12.7 N.m (1.0 ~ 1.3 kgf.m, 7.24 ~ 9.38 lbf.ft)