| VELOSTER(FS) >2012 > G 1.6 GDI > Body (Interior and Exterior) > Interior > Console>Repair procedures |

Replacement
Floor Console Replacement
[M/T]
• | A plastic trim tool is recommended, but if prying with a screwdriver, wrap it with protective tape, and apply protective tape around the related parts, to prevent damage.
• | Put on gloves to protect your hands.
1. | Using a screwdriver or remover, remove the parking brake cover (A).
2. | Using a screwdriver or remover, remove the gear boots (A).
3. | Using a screwdriver or remover, remove the console upper cover (A).
4. | Remove the console tray mat (A).
5. | After loosening the mounting screws and bolts, then remove the floor console assembly (A).
6. | After loosening the mounting clips and screws, then remove the console side cover (A).
7. | Installation is the reverse of removal.
• | Make sure the connector are connected in properly.
• | Replace any damage clips.
[A/T]
• | A plastic trim tool is recommended, but if prying with a screwdriver, wrap it with protective tape, and apply protective tape around the related parts, to prevent damage.
• | Put on gloves to protect your hands.
1. | Using a screwdriver or remover, remove the parking brake cover (A).
2. | Using a screwdriver or remover, remove the console upper cover (A).
3. | Disconnect the connector (A).
4. | Remove the console tray mat (A).
5. | After loosening the mounting screws and bolts, then remove the floor console assembly (A).
6. | After loosening the mounting clips and screws, then remove the console side cover (A).
7. | Installation is the reverse of removal.
• | Make sure the connectors are connected in properly.
• | Replace any damaged clips.
Rear Console Cover Replacement
• | A plastic trim tool is recommended, but if prying with a screwdriver, wrap it with protective tape, and apply protective tape around the related parts, to prevent damage.
• | Put on gloves to protect your hands.
1. | Using a screwdriver or remover, remove the rear console cover (A).
2. | Installation is the reverse of removal.
• | Replace any damage clips.
Armrest assembly Replacement
• | A plastic trim tool is recommended, but if prying with a screwdriver, wrap it with protective tape, and apply protective tape around the related parts, to prevent damage.
• | Put on gloves to protect your hands.
1. | Using a screwdriver or remover, remove the rear console cover (A).
2. | After loosening the mounting screws, then remove the armrest assembly (A).
3. | Installation is the reverse of removal.
• | Replace any damage clips.