| VELOSTER(FS) >2012 > G 1.6 GDI > Engine Mechanical System > Lubrication System > Oil Pan>Repair procedures |

Removal
1. | Remove the under covers (A).
Tightening torque: 6.9 ~ 10.8 N.m (0.7 ~ 1.1 kgf.m, 5.1 ~ 8.0 lb-ft)
2. | Drain engine oil.
3. | Using the SST(09215-3C000) and remove the oil pan.
• | Insert the SST between the oil pan and the ladder frame by tapping it with a plastic hammer in the direction of arrow.
• | After tapping the SST with a plastic hammer along the direction of arrow around more than 2/3 edge of the oil pan, remove it from the ladder frame.
• | Do not turn over the SST abruptly without tapping. It be result in damage of the SST.
Installation
1. | Install the oil pan.
(1) | Using a razor blade and gasket scraper, remove all the old packing material from the gasket surfaces.
Check that the mating surfaces are clean and dry before applying liquid gasket.
(2) | Apply liquid gasket as an even bead, centered between the edges of the mating surface.
Liquid gasket : TB 1217H or LOCTITE 5900H
• | To prevent leakage of oil, apply liquid gasket to the inner threads of the bolt holes.
• | Do not install the parts if five minutes or more have elapsed since applying the liquid gasket. Instead, reapply liquid gasket after removing the residue.
• | After assembly, wait at least 30 minutes before filling the engine with oil.
(3) | Install the oil pan (A) with the bolts. Uniformly tighten the bolts in several passes.
Tightening torque : 9.8 ~ 11.8N.m (1.0 ~ 1.2kgf.m, 7.2 ~ 8.7lb-ft)
2. | Refill engine oil.