| VELOSTER(FS) >2012 > G 1.6 GDI > Body Electrical System > Lighting System > High Mounted stop lamp>Repair procedures |

Removal
1. | Disconnect the negative(-) battery terminal.
2. | Remove the tailgate center trim. (Refer to the BD group - "Exterior - Tailgate")
3. | Loosen 4 nuts and remove the rear garnish assembly after disconnecting the connector.
4. | Loosen 5 screws and remove the garnish cover (A).
5. | Loosen 4 screws and remove the high mounted stop lamp (A).
Installation
1. | Install the high mounted stop lamp.
2. | Install the rear garnish and the tailgate trim.