| VELOSTER(FS) >2012 > G 1.6 GDI > Body Electrical System > Windshield Wiper/Washer > Windshield Wiper-Washer Switch>Repair procedures |

Inspection
Check for continuity between the terminals while operating the wiper and washer switch. If it is not normal condition, replace wiper and wiper switch.
Wiper Switch
Washer Switch
Removal
1. | Remove the steering column upper and lower shrouds (A) after removing 3 screws.
2. | Disconnect the connector(A).
3. | If necessary of removing the wiper & washer switch (A), release the lock of wiper switch using tool without removing the steering wheel and the clock spring.
4. | Remove the steering wheel. (Refer to the ST group - "Steering column and shaft")
5. | Remove the clock spring. (Refer to the RT group - "Airbag module")
6. | Remove the multifunction switch assembly(A) with 2 screws.
Installation
1. | Install the multifunction switch after connecting the connector.
2. | Install the clock spring and steering.
3. | Install the upper and lower shroud.
4. | Install the steering wheel.