| VELOSTER(FS) >2012 > G 1.6 GDI > Engine Mechanical System > Intake And Exhaust System > Muffler>Repair procedures |

Removal and Installation
1. | Disconnect the battery negative terminal.
Tightening torque Without battery sensor : 7.8 ~ 9.8 N.m (0.8 ~ 1.0 kgf.m, 5.8 ~ 7.2 lb-ft) With battery sensor : 4.0 ~ 6.0 N.m (0.4 ~ 0.6 kgf.m, 3.0 ~ 4.4 lb-ft)
2. | Disconnect the rear oxygen sensor connector (A).
3. | Remove the front muffler (A).
Tightening torque: 39.2 ~ 58.8 N.m (4.0 ~ 6.0 kgf.m, 28.9 ~ 43.4 lb-ft)
4. | Remove the center muffler (A).
Tightening torque: 39.2 ~ 58.8 N.m (4.0 ~ 6.0 kgf.m, 28.9 ~ 43.4 lb-ft)
5. | Remove the main muffler (A).
6. | Installation is the reverse order of removal.
When installing, replace with new gaskets.