| VELOSTER(FS) >2012 > G 1.6 GDI > Dual Clutch Transmission(DCT) System > Dual Clutch Transmission Control System > Gear Actuator>Repair procedures |

Removal
1. | Remove the following parts first:
A. | Air cleaner assembly and air duct (Refer to the Intake and Exhaust System of EM Group.)
B. | Battery and tray (Refer to the Charging System of EE Group.)
C. | ECM (Refer to the Engine Control Module of FL Group.)
2. | Place the shift lever in the N position.
3. | Disconnect the shift actuator connector (A) and select actuator connector (B), and then remove the wire fixing clip.
4. | Loosen the mounting bolt, and then remove the gear actuator (A).
Tightening torque: 19.6 ~ 26.5 N.m (2.0 ~ 2.7 kgf.m, 14.5 ~ 19.5 lb-ft)
Installation
1. | Installation is the reverse of removal.
• | Make sure that no debris falls into the hole (A).
• | Check the angle of the gear actuator finger (A), and also check whether the transmission lever is in the N position.