| VELOSTER(FS) >2012 > G 1.6 GDI > Body Electrical System > AVN System > AVN Remote Control>Repair procedures |

Inspection
1. | Check the audio remote control switch (A) for resistance between connector terminals in each switch position. [LH-AUDIO] [RH-TRIP] [Audio]
Switch | Connector terminal | Resistance (±5%)
Seek up | 3-5 | 430 Ω
Seek down | 3-5 | 1.11 kΩ
Mode | 3-5 | 2.11 kΩ
Volume up | 3-5 | 4.61 kΩ
Volume down | 3-5 | 6.81 kΩ
[Cruise]
Switch | Connector terminal | Resistance (±5%)
ON/ OFF | 3-4 | 880 Ω
Cancle | 3-4 | 180 Ω
SET - | 3-4 | 330 Ω
SET + | 3-4 | 550 Ω
[Bluetooth + Voice]
Switch | Connector terminal | Resistance (±5%)
Voice | 3-4 | 10.71 kΩ
End of call | 3-4 | 18.91 kΩ
Send | 3-4 | 40.91 kΩ
[Trip + Reset]
Switch | Connector terminal | Resistance (±5%)
Trip | 3-4 | 2.54 kΩ
Reset | 3-4 | 5.54 kΩ
Removal
1. | Disconnect the negative (-) battery terminal.
2. | Remove the driver airbag module. (Refer to the RT group - "Driver airbag module and clock spring")
3. | Remove the steering wheel. (Refer to the ST group - "Steering column & shaft")
4. | Remove the steering wheel cover (A) after loosening 4 screws.
5. | Remove the steering wheel remote control switches connectors. [LH-Audio/ Bluetooth + Voice] [RH-Cruise/ Trip + Reset]
6. | Remove the wiring and loosen 5 screws.
7. | Remove the steering wheel remote control switch assembly (A).
8. | Remove the bluetooth switch and the trip switch (A) after loosening the screws.
Installation
1. | Install the steering wheel remote control switch.
2. | Install the steering wheel cover.
3. | Install the steering wheel.
4. | Install the driver airbag module.
Make sure the audio remote control switch and the airbag module connectors are plugged in properly.