| VELOSTER(FS) >2012 > G 1.6 GDI > Body Electrical System > Smart key System > Smart key unit>Components and Components Location |

Component (1)
Connector Pin Information
No. | Connector A(26 pins) | No. | Connector B(16 pins) | No. | Connector C(22 pins)
1 | Battery power load | 1 | CAN L | 1 | Start/Stop button switch ILL
2 | - | 2 | CAN H | 2 | Immobilizer IND
3 | Power ground 1 | 3 | - | 3 | Start/Stop button LED OFF
4 | IGN 1 | 4 | Stop lamp fuse | 4 | Interior antenna #2 power
5 | IGN 1 relay | 5 | Brake switch | 5 | Interior antenna #1 power
6 | ACC | 6 | Immobilizer antenna power | 6 | -
7 | IGN 2 | 7 | - | 7 | -
8 | Start/Stop button switch 2 | 8 | Wheel speed | 8 | Trunk antenna power
9 | - | 9 | Driver toggle button | 9 | Bumper antenna power
10 | - | 10 | - | 10 | Assistant antenna power
11 | ESCL COM | 11 | External buzzer | 11 | Driver antenna power
12 | CAN H | 12 | P position / Clutch switch | 12 | SSB LED IGN
13 | CAN L | 13 | Start feedback | 13 | SSB illumination power
14 | Battery CPU | 14 | Immobilizer antenna ground | 14 | -
15 | - | 15 | Diagnostic - K | 15 | Interior antenna #2 ground
16 | Power ground 2 | 16 | Start/Stop button switch LED | 16 | Interior antenna #1 ground
17 | Starter relay |  |  | 17 | -
18 | IGN 2 relay | 18 | -
19 | ACC relay | 19 | Trunk antenna ground
20 | - | 20 | Bumper antenna ground
21 | Trunk lid switch | 21 | Assistant antenna ground
22 | - | 22 | Driver antenna ground
23 | RPM |  |
24 | EMS COM
25 | Start/Stop button switch 1
26 | Assistant toggle button