| VELOSTER(FS) >2012 > G 1.6 GDI > Dual Clutch Transmission(DCT) System > Dual Clutch Transmission Control System > Input Speed Sensor 1>Repair procedures |

Inspection
Refer to DTC code "P2765, P2766" Input Shaft Speed Sensor.
Removal
1. | Remove the under cover.
2. | Disconnect the input shaft speed sensor connector (A).
3. | Loosen the mounting bolt and then remove the input shaft speed sensor (B).
Installation
1. | Installation is the reverse of removal.
Tightening torque : 1.0 ~ 1.2 kgf.m