| VELOSTER(FS) >2012 > G 1.6 GDI > Body Electrical System > Seat Electrical > Seat Heater Switch>Repair procedures |

Removal
1. | Disconnect the negative (-) battery terminal.
2. | Remove the crash pad center fascia panel (A).
3. | Remove the driver and the assist seat heater switch connector, after loosening 4 screws.
Installation
1. | Install th driver and the assist seat heater switch connector.
2. | Install the crash pad ceter fascia panel.
3. | Connect the battery (-) terminal.
Inspection
Rear seat heater switch
1. | Disconnect the negative (-) battery terminal.
2. | Remove the crash pad center fascia panel.
3. | Disconnector the driver and the assist seat heater switch connector.
4. | Turn rear seat heater switch ON and check that continuity exists between the terminals.
5. | If there is no continuity, replace the seat heater switch.