| VELOSTER(FS) >2012 > G 1.6 GDI > Manual Transaxle System > General Information>Special Service Tools |

Special Service Tools
Tool (Number and name) | Illustration | Use
09200-38001,3N000 (Beam) 09200-4X000 (Adapter) 09200-2S100, 2S200 (Supporter) Engine support assembly |  | Removal and installation of the transaxle. Use assembling 09200-4X000 (Adapter) and 09200-2S100, 2S200 (Supporter) on 09200-38001, 3N000(Beam).
09200-3N000 Engine support fixture (Beam) |  | Removal and installation of the transaxle. Use this adapter (SST No. : 09200-4X000) with the supporter (SST No. : 09200-2S100, 2S200). ※Permit operating with 09200-38001.
09200-2S100 Engine support fixture (Supporter) |  | Removal and installation of the transaxle. Use this beam (SST No. : 09200-38001/3N000) with the supporter (SST No. : 09200-2S200) and adapter (SST No. : 09200-4X000).
09200-2S200 Engine support fixture (Supporter) |  | Removal and installation of the transaxle. Use this beam (SST No. : 09200-38001/3N000) with the adapter (SST No. : 09200-4X000) and supporter (SST No. : 09200-2S100).
09200-4X000 Engine support fixture (Adapter) |  | Removal and installation of the transaxle. Use this beam (SST No. : 09200-38001/3N000) with the supporter (SST No. : 09200-2S100, 2S000).